
XRD data files for this paper were collected between 05/02/2024 and 30/06/2026.  


For structure determination and phase purity data for the NMC samples were collected between 5 – 120o 2θ at 0.15 degree per minute on a PANanalytical Empyrean (Cu Kα). 


For structure determination and phase purity data for the NFM-333 samples were collected between 5 – 120o 2θ at 0.15 degree per minute on a Bruker D8 (Cu Kα). 

